
The front side of the glasses should provide protection against direct and scatter x-ray irradiation with the equivalent of 0.75mmPb lead and the side side 0.50mmPb lead. This issue will be documented by the company.
1. There should be a model that doctors who use glasses can wear over their glasses.
2. There will be a special carrying and storage box.
3. It should be a soft hair band that is adjustable in head width and can be attached and removed.
4. It should not fog up or obstruct vision during use.
5. It should be disinfectable and washable when necessary.
6. It should be disinfectable and washable when necessary.
7. It must be made of impact-resistant material.
8. The glasses are full protection models and should block the rays coming from both the front and the sides.
9. The protective properties and protection rates of the glasses against X-rays must be documented with the test results.
10. X-ray protective lead glasses must be produced and certified in accordance with the Personal Protective Equipment Regulation (Official Gazette dated 01 May 2019 and numbered 30761, new regulation (EU) 2016/425 x personal protection directive).
11. Different models should be offered upon hospital request.




