LENFPED TECHNICAL SPECIFICATION

1- It should be ideally manufactured to provide a suitable combination on protective aprons.
2- Lymphpads must be manufactured to provide protection against secondary ionization radiation against ambient radiation.
3- It should be produced with an injection closure system for comfortable use by the user.
4- In accordance with body ergonomics, they must be produced using flexible hydroair material that prevents sweating and is breathable.
5- It should be ideally manufactured to provide a suitable combination on protective aprons.
6- It should be made of Hydro Air material that will cover the shoulder and back area well and should not cause sweating.
7- It should provide protection on the Lymph Areas and Biceps Area.
8- It should be made of Hydro Air material that will cover the shoulder and back area well and should not cause sweating.
9- It should provide protection on the Lymph Areas and Biceps Area.
10- Products must be covered by a 2-year warranty against production and fabrication defects.
11- Companies should provide a single hanger with the product for easy storage of LENFEDs.
12- There should be color options upon user request.
13- There should be color options upon user request.
14- The product must have a label showing its production date and protective properties.
15- The manufacturer must have ISO 9001 certificate and ISO 13485 certificate.

