




LONG HANDLE NUCLEAR LEAD GLOVE




1. X-Ray protective lead gloves should provide maximum protection to the user's hands against radiation.
2. Its weight should be such that it does not disturb the user.
3. Its weight should be such that it does not disturb the user.
4. The surface must be cleanable with a wet cloth.
5. There should not be any breakage or deformation when folded.
6. The product must have a module c2 and module b certificate.
7. It must have a lead thickness of 0.50 mm pb
8. The product must have a module c2 and module b certificate.
9. The company must have an ISO 9001:2015 certificate.
10. The company must have an ISO 13485:2016 certificate. This must be presented upon delivery of the material.
11. There must be full approval and test reports for the production of the product. It should offer this when requested. A report showing at least 96% protection of the product must be submitted with the product.
12. Evaluations should be made on samples.


