
PANORAMIC MASK TECHNICAL SPECIFICATION
1. The panoramic mask should be supplied protected with its special case.
2. Panoramic mask must provide at least 1 mm PB protection.
3. The panoramic mask is designed to adapt to all types of faces.
4. It should provide a clear image due to its transparent feature.
5. There should be a support cover on the forehead to protect the forehead.
6. The product must be produced and certified in accordance with the Personal Protective Equipment Regulation (Official Gazette dated 01 May 2019 and numbered 30761, new regulation (EU) 2016/425 x personal protection directive).
7. The product must be produced and certified in accordance with the Personal Protective Equipment Regulation (Official Gazette dated 01 May 2019 and numbered 30761, new regulation (EU) 2016/425 x personal protection directive).
8. The adjustable mechanism must be sturdy.
9. It is produced with a non-chipping protector against breakage and disintegration.
10. It cannot be deleted.
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