
The front side of the glasses should provide protection against direct and scatter x-ray irradiation with the equivalent of 0.75mmPb lead and the side side 0.50mmPb lead. This issue will be documented by the company.
1. The front side of the glasses should provide protection against direct and scatter x-ray irradiation with the equivalent of 0.75mmPb lead and the side side 0.50mmPb lead. This issue will be documented by the company.
2. It should be a soft hair band that is adjustable in head width and can be attached and removed.
3. It should not fog up or obstruct vision during use.
4. It must be made of impact-resistant material.
5. It must be made of impact-resistant material.
6. The protective properties and protection rates of the glasses against X-rays must be documented with the test results.
7. The glasses are full protection models and should block the rays coming from both the front and the sides.
8. In line with the old standards for products, Article 11A, Article 11B documents should not be submitted. These documents have become obsolete and documents must be submitted for the sale of products certified according to the new revision.
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11. Different models should be offered upon hospital request.




