
The visor must be made of radiation protective equipment.
1. The visor must be made of radiation protective equipment.
2. The visor should cover most of the face.
3. The leaded acrylic mask should have a length of 20 cm (+-5 cm) from the top to the bottom.
4. It should be easily cleanable with a soft cloth without irritation.
5. The sponge on the front of the headband should lighten the weight.
6. The size should be standard and thus adapt to every face type.
7. The glass structure must be resistant to breakage, and even if it breaks, the glass must have the feature of not shattering.
8. The glass structure must be resistant to breakage, and even if it breaks, the glass must have the feature of not shattering.



