

It should be a model specially designed and produced for lead aprons.
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1- It should be a model specially designed and produced for lead aprons.
2- It must be manufactured with a capacity to carry a lead apron.
3- It must be of wooden construction, durable and suitable for hospital use.
4- It must be ISO 9001:2008 quality certified.
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