The lead coating must be designed to not interfere with the vehicle's functions.

1. The lead coating must be designed to not interfere with the vehicle's functions.
2. It is necessary to use lead material that protects against radiation in the coating of the vehicle.
3. It is necessary to use lead material that protects against radiation in the coating of the vehicle.
4. All operations will be carried out on the vehicle, and if the vehicle comes and goes when necessary, the expenses will be covered by the company.
5. Protective material must be removable when necessary.
6. Protective material must be removable when necessary.
7. In-vehicle measurements of the area where the protective material will be applied will be taken by the company and will be made as requested by the institution.
8. Personal Protective Equipment Regulation (Official Gazette dated 01 May 2019 and numbered 30761, New Regulation (EU) 2016/425 He must accept it.
9. There Must Be TAEK Approval and Test Reports for the Production of the Product. Must Offer This When Requested.
10. There must be an ISO 45001:2018 certificate for the production of radiation protective products, which is internationally valid, from an accredited institution for the production of the product.
11. There must be an ISO 45001:2018 certificate for the production of radiation protective products, which is internationally valid, from an accredited institution for the production of the product.
12. The manufacturer must provide a 2 (two) year warranty against manufacturing defects.
13. The manufacturer must provide a 2 (two) year warranty against manufacturing defects.

