
X-Ray protective lead gloves should provide maximum protection to the user's hands against radiation.

1. X-Ray protective lead gloves should provide maximum protection to the user's hands against radiation.
2. Its weight should be such that it does not disturb the user.
3. The surface must be cleanable with a wet cloth.
4. The surface must be cleanable with a wet cloth.
5. The packaging must contain original information indicating the manufacturer's information and protective norms.
6. The packaging must contain original information indicating the manufacturer's information and protective norms.
7. The company must have an ISO 9001:2015 certificate.
8. The company must have an ISO 13485:2016 certificate. This must be presented upon delivery of the material.
9. The company must have an ISO 13485:2016 certificate. This must be presented upon delivery of the material.
10. The gloves are certified according to directive 2016/425EU category III and have a 4-digit CE certificate obtained from a Notified Body.
11. Radiation protective gloves should be powder-free. If you want to use powder when wearing it, the powder should be presented in its original packaging.
12. There must be an ISO 45001:2018 certificate.
13. Protective Gloves must be certified according to EN 420:2003 + A1:2009 standard and EN 374-2:2003 standard and this must be submitted to the institution with the documents related to the manufacturer.
14. Protective Gloves must be certified according to EN 420:2003 + A1:2009 standard and EN 374-2:2003 standard and this must be submitted to the institution with the documents related to the manufacturer.
15. It should be in various sizes. ( 6.5- 7- 7.5 -8 -8.5- 9 )
16. If the company selling the product is a Distributor, it must submit a Distributorship Certificate; if it is not a Distributor, it must submit an authorized dealer certificate obtained from the Distributor or the manufacturer, and issued based on the relevant purchase addressed to our institution.
17. A commitment to comply with the specification must be written stating that all specification articles are complied with.
18. Evaluations should be made on samples.


