PATIENT AND STAFF PROTECTION PORTABLE LEAD CURTAIN SPECIFICATION

1. The system does not have the ability to move.
2. There must be a channel on the system that helps it rise and fall.
3. The system must be fixed with at least 4 wheels.
4. The curtain to be mounted on the system must serve the purpose of protection.
5. In intensive care units, it should act as a curtain between two patients or between the user and the patient.
6. It must have 0.50 mm pb lead equivalent.
7. Upon request, the manufacturer should have different sizes in line with the user's request. These dimensions must be presented at the time of request.
8. The curtain must have a minimum width and height. (+-)
9. Upon request, the manufacturer should have different sizes in line with the user's request. These dimensions must be presented at the time of request.
10. Upon request, the manufacturer should have different sizes in line with the user's request. These dimensions must be presented at the time of request.
11. The user should be able to shoot and view from behind the protector when necessary, and to protect himself by using the moving parts left and right.
12. The protective curtain must be made of leather. The skin color will be determined by the institution. It should be deletable and have this structure.
13. The protective system is produced against rust.
14. Regarding Protective Curtains, Personal Protective Equipment Regulation (Official Gazette dated 01 May 2019 and numbered 30761, New Regulation (EU) 2016/425 It must.
15. Articel 11 A Articel 11 B Certificate Should Not Be Submitted in Line with Old Standards for Products. These Documents Have Lost Their Validity, and Documents Must Be Submitted for the Sale of Products Certified According to the New Revision.
16. The Seller Company Must Provide a Work Experience Certificate or Reference Regarding Previous Works It Has Done, If Requested by the Institution Regarding the Products.
17. The manufacturer must have an ISO 9001:2015 certificate.
18. Demo and practical references must be submitted during the request.


